**AIM :** to create a Control of Fan, Light, Window & Application of Using Cisco Packet Tracer .

step1:-first take Home gateway

step2:- link that gateway to the home appliance like celling fan , lamp ,window and coffee maker make a connection between the appliances and home gateway

step3:-connect that gateway to the appliances and change the IP address in it

step4:- after connection check the IP address of the all gateway and appliances in the config

step5:- if command send correctly you got successfull other wise recheck the connections

Step6:- Then the Control of Fan, Light, Window & Application of Using Cisco Packet Tracer was successfully simulated .

.



